#50950 FACE SHIELD – INSTRUCTIONS FOR USE

1. PEEL MASKING OFF BOTH SIDES OF CLEAR SHIELD
2. ATTACH MIDDLE LOCATOR HOLE ON CLEAR SHIELD TO MDDLE LOCATOR POINT ON FRONT OF HEADBAND
3. PUSH FIRMLY OVER EACH LOCATOR POINT MOVING FROM CENTRE OUTWARDS
4. USING ADJUSTABLE ELASTIC, ADJUST HEADBAND TO FIT
5. ADJUST FRONT OF HEADBAND FRAME UP OR DOWN FOR BEST FIT AND ENSURE CLEAR SHIELD COVERS MOUTH

